From a6a49b7ab0984b39ae7c8d0db093ce109c8f8281 Mon Sep 17 00:00:00 2001
From: "Matthias P. Braendli" <matthias.braendli@mpb.li>
Date: Sun, 22 Mar 2015 20:28:21 +0100
Subject: Add scenarios content

---
 interfaces.tex | 1 +
 1 file changed, 1 insertion(+)

(limited to 'interfaces.tex')

diff --git a/interfaces.tex b/interfaces.tex
index 1c7512e..41bf72d 100644
--- a/interfaces.tex
+++ b/interfaces.tex
@@ -122,6 +122,7 @@ computers, but it is not necessary. It is also possible, and even encouraged to
 use this interconnection locally on the same machine.
 
 \subsubsection{Between Encoder and Multiplexer}
+\label{sec:between_encoder_and_multiplexer}
 
 Between FDK-AAC-DABplus and ODR-DabMux, the ZeroMQ connection transmits AAC
 superframes, with additional metadata that contains the audio level indication
-- 
cgit v1.2.3

