From 1fe1be7de91b011e24be0f773f7003adc54078d9 Mon Sep 17 00:00:00 2001
From: "Matthias P. Braendli" <matthias.braendli@mpb.li>
Date: Fri, 2 May 2014 15:31:11 +0200
Subject: Introduction and Origins

---
 appendix.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'appendix.tex')

diff --git a/appendix.tex b/appendix.tex
index e366e7f..fd2169e 100644
--- a/appendix.tex
+++ b/appendix.tex
@@ -1,14 +1,14 @@
 
-\section{CRC-DABMUX ETI file formats}
+\section{ODR-DabMux ETI file formats}
 \label{etiformat}
-CRC-DABMUX supports three output formats for the ETI stream, that have been described on the mmbTools forum
+ODR-DabMux supports three output formats for the ETI stream, that have been described on the mmbTools forum
 website.\footnote{\url{http://mmbtools.crc.ca/component/option,com\_fireboard/Itemid,55/func,view/id,4/catid,13/\#28}}
 
 The three formats are called \emph{framed}, \emph{streamed} and \emph{raw}.
 
 The \emph{framed} format is used for saving a finite ETI stream into a file. Each frame does not contain any padding, and the
 format can be described as follows:
-\begin{lstlisting} 
+\begin{lstlisting}
 uint32_t nbFrames
 // for each frame
   uint16_t frameSize
@@ -17,7 +17,7 @@ uint32_t nbFrames
 
 When streaming data, in which case the number of frames is not known in advance, the \emph{streamed} format can be used.
 This format is identical to the first one except for the missing \texttt{nbFrames}.
-\begin{lstlisting} 
+\begin{lstlisting}
 // for each frame
   uint16_t frameSize
   uint8_t data[frameSize]
@@ -25,7 +25,7 @@ This format is identical to the first one except for the missing \texttt{nbFrame
 
 The \emph{raw} format corresponds to ETI(NI), where each frame has a constant size of 6144 Bytes. The padding in this
 case is necessary.
-\begin{lstlisting} 
+\begin{lstlisting}
 // for each frame
   uint8_t data[6144]
 \end{lstlisting}
-- 
cgit v1.2.3

