From 94e856a32ac95faed7b6e66b5b6918f3979f5e80 Mon Sep 17 00:00:00 2001
From: "Matthias P. Braendli" <matthias.braendli@mpb.li>
Date: Tue, 19 Jul 2022 17:09:40 +0200
Subject: Apply minor changes

---
 scenarios.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'scenarios.tex')

diff --git a/scenarios.tex b/scenarios.tex
index 3afbaa8..f28611b 100644
--- a/scenarios.tex
+++ b/scenarios.tex
@@ -337,8 +337,8 @@ new infrastructure if the stream is of good quality. The main disadvantage is
 that the audio is encoded twice, and this coding cascading degrades the audio
 quality.
 
-Often, web-streams are encoded in mp3 at $44100\Hz$ sample-rate, whereas DAB
-is most often $48000\Hz$ or sometimes $32000\Hz$. A sample-rate conversion is
+Often, web-streams are encoded in mp3 at $44100$Hz sample-rate, whereas DAB
+is most often $48000$Hz or sometimes $32000$Hz. A sample-rate conversion is
 necessary in the stream decoder.
 
 There are many different stream decoders, and gstreamer, mpg123 and mplayer have
-- 
cgit v1.2.3

